#MicroXplorer Configuration settings - do not modify
ADC1.Channel-2\#ChannelRegularConversion=ADC_CHANNEL_10
ADC1.ContinuousConvMode=DISABLE
ADC1.EnableInjectedConversion=DISABLE
ADC1.EnableRegularConversion=ENABLE
ADC1.ExternalTrigConv=ADC_EXTERNALTRIGCONV_T3_TRGO
ADC1.IPParameters=ContinuousConvMode,EnableRegularConversion,EnableInjectedConversion,InjNumberOfConversion,Rank-2\#ChannelRegularConversion,Channel-2\#ChannelRegularConversion,SamplingTime-2\#ChannelRegularConversion,NbrOfConversionFlag,master,ExternalTrigConv
ADC1.InjNumberOfConversion=0
ADC1.NbrOfConversionFlag=1
ADC1.Rank-2\#ChannelRegularConversion=1
ADC1.SamplingTime-2\#ChannelRegularConversion=ADC_SAMPLETIME_1CYCLE_5
ADC1.master=1
CAD.formats=[]
CAD.pinconfig=Dual
CAD.provider=
Dma.ADC1.0.Direction=DMA_PERIPH_TO_MEMORY
Dma.ADC1.0.Instance=DMA1_Channel1
Dma.ADC1.0.MemDataAlignment=DMA_MDATAALIGN_HALFWORD
Dma.ADC1.0.MemInc=DMA_MINC_ENABLE
Dma.ADC1.0.Mode=DMA_CIRCULAR
Dma.ADC1.0.PeriphDataAlignment=DMA_PDATAALIGN_HALFWORD
Dma.ADC1.0.PeriphInc=DMA_PINC_DISABLE
Dma.ADC1.0.Priority=DMA_PRIORITY_VERY_HIGH
Dma.ADC1.0.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority
Dma.Request0=ADC1
Dma.RequestsNb=1
File.Version=6
GPIO.groupedBy=Group By Peripherals
I2C2.GeneralCallMode=I2C_GENERALCALL_ENABLE
I2C2.IPParameters=GeneralCallMode
KeepUserPlacement=false
Mcu.CPN=STM32F103ZET6
Mcu.Family=STM32F1
Mcu.IP0=ADC1
Mcu.IP1=DMA
Mcu.IP10=TIM4
Mcu.IP11=UART5
Mcu.IP12=USART1
Mcu.IP13=USART2
Mcu.IP14=USART3
Mcu.IP2=I2C2
Mcu.IP3=NVIC
Mcu.IP4=RCC
Mcu.IP5=SPI3
Mcu.IP6=SYS
Mcu.IP7=TIM1
Mcu.IP8=TIM2
Mcu.IP9=TIM3
Mcu.IPNb=15
Mcu.Name=STM32F103Z(C-D-E)Tx
Mcu.Package=LQFP144
Mcu.Pin0=PE5
Mcu.Pin1=PE6
Mcu.Pin10=PA3
Mcu.Pin11=PB10
Mcu.Pin12=PB11
Mcu.Pin13=PB13
Mcu.Pin14=PD15
Mcu.Pin15=PA8
Mcu.Pin16=PA9
Mcu.Pin17=PA10
Mcu.Pin18=PA13
Mcu.Pin19=PA14
Mcu.Pin2=PC14-OSC32_IN
Mcu.Pin20=PC10
Mcu.Pin21=PC11
Mcu.Pin22=PC12
Mcu.Pin23=PD2
Mcu.Pin24=PD5
Mcu.Pin25=PB3
Mcu.Pin26=PB4
Mcu.Pin27=PB5
Mcu.Pin28=PB7
Mcu.Pin29=VP_SYS_VS_tim8
Mcu.Pin3=PC15-OSC32_OUT
Mcu.Pin30=VP_TIM3_VS_ClockSourceINT
Mcu.Pin31=VP_TIM4_VS_ClockSourceINT
Mcu.Pin32=VP_RealThread.X-CUBE-RT-Thread_Nano_VS_RTOSJjRTAaThread_4.1.1_4.1.1
Mcu.Pin33=VP_STMicroelectronics.X-CUBE-ALGOBUILD_VS_DSPOoLibraryJjLibrary_1.4.0_1.4.0
Mcu.Pin4=OSC_IN
Mcu.Pin5=OSC_OUT
Mcu.Pin6=PC0
Mcu.Pin7=PA0-WKUP
Mcu.Pin8=PA1
Mcu.Pin9=PA2
Mcu.PinsNb=34
Mcu.ThirdParty0=RealThread.X-CUBE-RT-Thread_Nano.4.1.1
Mcu.ThirdParty1=STMicroelectronics.X-CUBE-ALGOBUILD.1.4.0
Mcu.ThirdPartyNb=2
Mcu.UserConstants=TEC_DEAD_TIME,100;AD7793_SPI,$$_SPI3_IP_HANDLE_$$;RS485_COM,$$_UART5_IP_HANDLE_$$;TEC_TIM_COUNTER,143;SAMPLING_TIM_PRE,71;US_TIM_PERIOD_COUNT,9999;TEC_TIM_PRESCALER,99;TEC_TIM,$$_TIM1_IP_HANDLE_$$;HMI_COM,$$_USART2_IP_HANDLE_$$;SAMPLING_TIM,$$_TIM3_IP_HANDLE_$$;US_TIM_PRE,71;TIMESTAMP_TIM,$$_TIM4_IP_HANDLE_$$;ENCODER_TIM,$$_TIM2_IP_HANDLE_$$;SAMPLING_TIM_PERIOD_COUNT,877;SERVO_COM,$$_USART3_IP_HANDLE_$$;LIGHT_ADC,$$_ADC1_IP_HANDLE_$$;ENCODER_MAX_COUNT,65535
Mcu.UserName=STM32F103ZETx
MxCube.Version=6.15.0
MxDb.Version=DB.6.0.150
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.DMA1_Channel1_IRQn=true\:0\:0\:false\:false\:true\:true\:false\:true\:true
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:false\:false\:false\:false\:false
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.PendSV_IRQn=true\:0\:0\:false\:false\:false\:false\:false\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:false\:false\:false\:false\:false
NVIC.SavedPendsvIrqHandlerGenerated=false
NVIC.SavedSvcallIrqHandlerGenerated=false
NVIC.SavedSystickIrqHandlerGenerated=false
NVIC.SysTick_IRQn=true\:0\:0\:false\:false\:false\:false\:false\:true\:false
NVIC.TIM2_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:true\:true
NVIC.TIM3_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:true\:true
NVIC.TIM4_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:true\:true
NVIC.TIM8_UP_IRQn=true\:15\:0\:false\:false\:true\:false\:false\:true\:true
NVIC.TimeBase=TIM8_UP_IRQn
NVIC.TimeBaseIP=TIM8
NVIC.UART5_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:true\:true
NVIC.USART1_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:true\:true
NVIC.USART2_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:true\:true
NVIC.USART3_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:true\:true
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
OSC_IN.Mode=HSE-External-Oscillator
OSC_IN.Signal=RCC_OSC_IN
OSC_OUT.Mode=HSE-External-Oscillator
OSC_OUT.Signal=RCC_OSC_OUT
PA0-WKUP.GPIOParameters=GPIO_Label
PA0-WKUP.GPIO_Label=TIM2_ENCODER_B
PA0-WKUP.Signal=S_TIM2_CH1_ETR
PA1.GPIOParameters=GPIO_Label
PA1.GPIO_Label=TIM2_ENCODER_A
PA1.Signal=S_TIM2_CH2
PA10.GPIOParameters=GPIO_Label
PA10.GPIO_Label=UART1_LCD_RX
PA10.Mode=Asynchronous
PA10.Signal=USART1_RX
PA13.Mode=Serial_Wire
PA13.Signal=SYS_JTMS-SWDIO
PA14.Mode=Serial_Wire
PA14.Signal=SYS_JTCK-SWCLK
PA2.GPIOParameters=GPIO_Label
PA2.GPIO_Label=UART2_TX_LCD
PA2.Mode=Asynchronous
PA2.Signal=USART2_TX
PA3.GPIOParameters=GPIO_Label
PA3.GPIO_Label=UART2_RX_LCD
PA3.Mode=Asynchronous
PA3.Signal=USART2_RX
PA8.GPIOParameters=GPIO_Speed,GPIO_Label
PA8.GPIO_Label=TIM1_CH1_TEC
PA8.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PA8.Locked=true
PA8.Signal=S_TIM1_CH1
PA9.GPIOParameters=GPIO_Label
PA9.GPIO_Label=UART1_LCD_TX
PA9.Locked=true
PA9.Mode=Asynchronous
PA9.Signal=USART1_TX
PB10.GPIOParameters=GPIO_Label
PB10.GPIO_Label=I2C2_EEPROM_SCL
PB10.Locked=true
PB10.Mode=I2C
PB10.Signal=I2C2_SCL
PB11.GPIOParameters=GPIO_Label
PB11.GPIO_Label=I2C2_EEPROM_SDA
PB11.Locked=true
PB11.Mode=I2C
PB11.Signal=I2C2_SDA
PB13.GPIOParameters=GPIO_Speed,GPIO_Label
PB13.GPIO_Label=TIM1_CH1N_TEC
PB13.GPIO_Speed=GPIO_SPEED_FREQ_HIGH
PB13.Locked=true
PB13.Mode=PWM Generation1 CH1 CH1N
PB13.Signal=TIM1_CH1N
PB3.GPIOParameters=GPIO_Label
PB3.GPIO_Label=SPI3_SCK_AD7793
PB3.Mode=Full_Duplex_Master
PB3.Signal=SPI3_SCK
PB4.GPIOParameters=GPIO_Label
PB4.GPIO_Label=SPI3_MISO_AD7793
PB4.Mode=Full_Duplex_Master
PB4.Signal=SPI3_MISO
PB5.GPIOParameters=GPIO_Label
PB5.GPIO_Label=SPI3_MOSI_AD7793
PB5.Mode=Full_Duplex_Master
PB5.Signal=SPI3_MOSI
PB7.GPIOParameters=GPIO_Label
PB7.GPIO_Label=SPI3_CS_AD7793
PB7.Locked=true
PB7.Signal=GPIO_Output
PC0.Locked=true
PC0.Signal=ADCx_IN10
PC10.GPIOParameters=GPIO_Label
PC10.GPIO_Label=UART3_SERVO_TX
PC10.Locked=true
PC10.Mode=Asynchronous
PC10.Signal=USART3_TX
PC11.GPIOParameters=GPIO_Label
PC11.GPIO_Label=UART3_SERVO_RX
PC11.Locked=true
PC11.Mode=Asynchronous
PC11.Signal=USART3_RX
PC12.GPIOParameters=GPIO_Label
PC12.GPIO_Label=UART5_RS485_TX
PC12.Mode=Asynchronous
PC12.Signal=UART5_TX
PC14-OSC32_IN.Mode=LSE-External-Oscillator
PC14-OSC32_IN.Signal=RCC_OSC32_IN
PC15-OSC32_OUT.Mode=LSE-External-Oscillator
PC15-OSC32_OUT.Signal=RCC_OSC32_OUT
PD15.GPIOParameters=GPIO_Label
PD15.GPIO_Label=FAN_CTRL
PD15.Locked=true
PD15.Signal=GPIO_Output
PD2.GPIOParameters=GPIO_Label
PD2.GPIO_Label=UART5_RS485_RX
PD2.Locked=true
PD2.Mode=Asynchronous
PD2.Signal=UART5_RX
PD5.GPIOParameters=GPIO_Label
PD5.GPIO_Label=FAN_CONTROL
PD5.Locked=true
PD5.Signal=GPIO_Output
PE5.GPIOParameters=GPIO_Speed,PinState,GPIO_PuPd,GPIO_Label
PE5.GPIO_Label=PE5_LED1
PE5.GPIO_PuPd=GPIO_NOPULL
PE5.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PE5.Locked=true
PE5.PinState=GPIO_PIN_SET
PE5.Signal=GPIO_Output
PE6.GPIOParameters=PinState,GPIO_Label
PE6.GPIO_Label=PE6_LED2
PE6.Locked=true
PE6.PinState=GPIO_PIN_SET
PE6.Signal=GPIO_Output
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerLinker=GCC
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=true
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32F103ZETx
ProjectManager.FirmwarePackage=STM32Cube FW_F1 V1.8.6
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=polarimeter.ioc
ProjectManager.ProjectName=polarimeter
ProjectManager.ProjectStructure=
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=CMake
ProjectManager.TemplateDestinationPath=E\:\\project\\polarimeter
ProjectManager.TemplateSourcePath=D\:\\Program Files\\STMicroelectronics\\STM32Cube\\STM32CubeMX\\db\\extra_templates
ProjectManager.ToolChainLocation=
ProjectManager.UAScriptAfterPath=
ProjectManager.UAScriptBeforePath=
ProjectManager.UnderRoot=false
ProjectManager.functionlistsort=1-SystemClock_Config-RCC-true-HAL-false,2-MX_GPIO_Init-GPIO-true-HAL-true,3-MX_DMA_Init-DMA-false-HAL-true,4-MX_I2C2_Init-I2C2-true-HAL-true,5-MX_USART1_UART_Init-USART1-true-HAL-true,6-MX_USART2_UART_Init-USART2-true-HAL-true,7-MX_UART5_Init-UART5-true-HAL-true,8-MX_USART3_UART_Init-USART3-true-HAL-true,9-MX_TIM1_Init-TIM1-true-HAL-true,10-MX_SPI3_Init-SPI3-true-HAL-true,11-MX_ADC1_Init-ADC1-true-HAL-true,12-MX_TIM2_Init-TIM2-true-HAL-true,13-MX_TIM3_Init-TIM3-true-HAL-true,14-MX_TIM4_Init-TIM4-true-HAL-true
RCC.ADCFreqValue=12000000
RCC.ADCPresc=RCC_ADCPCLK2_DIV6
RCC.AHBFreq_Value=72000000
RCC.APB1CLKDivider=RCC_HCLK_DIV2
RCC.APB1Freq_Value=36000000
RCC.APB1TimFreq_Value=72000000
RCC.APB2Freq_Value=72000000
RCC.APB2TimFreq_Value=72000000
RCC.FCLKCortexFreq_Value=72000000
RCC.FSMCFreq_Value=72000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=72000000
RCC.I2S2Freq_Value=72000000
RCC.I2S3Freq_Value=72000000
RCC.IPParameters=ADCFreqValue,ADCPresc,AHBFreq_Value,APB1CLKDivider,APB1Freq_Value,APB1TimFreq_Value,APB2Freq_Value,APB2TimFreq_Value,FCLKCortexFreq_Value,FSMCFreq_Value,FamilyName,HCLKFreq_Value,I2S2Freq_Value,I2S3Freq_Value,MCOFreq_Value,PLLCLKFreq_Value,PLLMCOFreq_Value,PLLMUL,PLLSourceVirtual,SDIOFreq_Value,SDIOHCLKDiv2FreqValue,SYSCLKFreq_VALUE,SYSCLKSource,TimSysFreq_Value,USBFreq_Value,VCOOutput2Freq_Value
RCC.MCOFreq_Value=72000000
RCC.PLLCLKFreq_Value=72000000
RCC.PLLMCOFreq_Value=36000000
RCC.PLLMUL=RCC_PLL_MUL9
RCC.PLLSourceVirtual=RCC_PLLSOURCE_HSE
RCC.SDIOFreq_Value=72000000
RCC.SDIOHCLKDiv2FreqValue=36000000
RCC.SYSCLKFreq_VALUE=72000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.TimSysFreq_Value=72000000
RCC.USBFreq_Value=72000000
RCC.VCOOutput2Freq_Value=8000000
RealThread.X-CUBE-RT-Thread_Nano.4.1.1.IPParameters=RT_USING_MUTEX,RT_USING_EVENT,RT_USING_SIGNALS,RT_USING_FINSH,RT_USING_HEAP,RT_MAIN_THREAD_STACK_SIZE,RT_USING_OVERFLOW_CHECK,RT_USING_MESSAGEQUEUE,RT_USING_SMALL_MEM_AS_HEAP,RT_USING_SMALL_MEM,RTAaThreadCcRTOSJjkernel,RTAaThreadCcRTOSJjshell,RTAaThreadCcRTOSJjlibcpu
RealThread.X-CUBE-RT-Thread_Nano.4.1.1.RTAaThreadCcRTOSJjkernel=true
RealThread.X-CUBE-RT-Thread_Nano.4.1.1.RTAaThreadCcRTOSJjlibcpu=true
RealThread.X-CUBE-RT-Thread_Nano.4.1.1.RTAaThreadCcRTOSJjshell=true
RealThread.X-CUBE-RT-Thread_Nano.4.1.1.RTOSJjRTAaThread_Checked=true
RealThread.X-CUBE-RT-Thread_Nano.4.1.1.RT_MAIN_THREAD_STACK_SIZE=4086
RealThread.X-CUBE-RT-Thread_Nano.4.1.1.RT_USING_EVENT=1
RealThread.X-CUBE-RT-Thread_Nano.4.1.1.RT_USING_FINSH=0
RealThread.X-CUBE-RT-Thread_Nano.4.1.1.RT_USING_HEAP=1
RealThread.X-CUBE-RT-Thread_Nano.4.1.1.RT_USING_MESSAGEQUEUE=1
RealThread.X-CUBE-RT-Thread_Nano.4.1.1.RT_USING_MUTEX=1
RealThread.X-CUBE-RT-Thread_Nano.4.1.1.RT_USING_OVERFLOW_CHECK=1
RealThread.X-CUBE-RT-Thread_Nano.4.1.1.RT_USING_SIGNALS=0
RealThread.X-CUBE-RT-Thread_Nano.4.1.1.RT_USING_SMALL_MEM=1
RealThread.X-CUBE-RT-Thread_Nano.4.1.1.RT_USING_SMALL_MEM_AS_HEAP=1
RealThread.X-CUBE-RT-Thread_Nano.4.1.1_SwParameter=RTAaThreadCcRTOSJjshell\:true;RTAaThreadCcRTOSJjlibcpu\:true;RTAaThreadCcRTOSJjkernel\:true;
SH.ADCx_IN10.0=ADC1_IN10,IN10
SH.ADCx_IN10.ConfNb=1
SH.S_TIM1_CH1.0=TIM1_CH1,PWM Generation1 CH1 CH1N
SH.S_TIM1_CH1.ConfNb=1
SH.S_TIM2_CH1_ETR.0=TIM2_CH1,Encoder_Interface
SH.S_TIM2_CH1_ETR.ConfNb=1
SH.S_TIM2_CH2.0=TIM2_CH2,Encoder_Interface
SH.S_TIM2_CH2.ConfNb=1
SPI3.BaudRatePrescaler=SPI_BAUDRATEPRESCALER_16
SPI3.CLKPhase=SPI_PHASE_2EDGE
SPI3.CLKPolarity=SPI_POLARITY_HIGH
SPI3.CalculateBaudRate=2.25 MBits/s
SPI3.Direction=SPI_DIRECTION_2LINES
SPI3.IPParameters=VirtualType,Mode,Direction,CalculateBaudRate,CLKPolarity,CLKPhase,BaudRatePrescaler
SPI3.Mode=SPI_MODE_MASTER
SPI3.VirtualType=VM_MASTER
STMicroelectronics.X-CUBE-ALGOBUILD.1.4.0.DSPOoLibraryJjLibrary_Checked=true
STMicroelectronics.X-CUBE-ALGOBUILD.1.4.0.IPParameters=LibraryCcDSPOoLibraryJjDSPOoLibrary
STMicroelectronics.X-CUBE-ALGOBUILD.1.4.0.LibraryCcDSPOoLibraryJjDSPOoLibrary=true
STMicroelectronics.X-CUBE-ALGOBUILD.1.4.0_SwParameter=LibraryCcDSPOoLibraryJjDSPOoLibrary\:true;
TIM1.AutoReloadPreload=TIM_AUTORELOAD_PRELOAD_ENABLE
TIM1.Channel-PWM\ Generation1\ CH1\ CH1N=TIM_CHANNEL_1
TIM1.DeadTime=TEC_DEAD_TIME
TIM1.IPParameters=Channel-PWM Generation1 CH1 CH1N,Period,Prescaler,AutoReloadPreload,DeadTime,OCNPolarity_1,OCNIdleState_1
TIM1.OCNIdleState_1=TIM_OCNIDLESTATE_RESET
TIM1.OCNPolarity_1=TIM_OCNPOLARITY_HIGH
TIM1.Period=TEC_TIM_COUNTER
TIM1.Prescaler=TEC_TIM_PRESCALER
TIM2.AutoReloadPreload=TIM_AUTORELOAD_PRELOAD_ENABLE
TIM2.EncoderMode=TIM_ENCODERMODE_TI12
TIM2.IC1Filter=6
TIM2.IC2Filter=6
TIM2.IPParameters=EncoderMode,TIM_MasterSlaveMode,TIM_MasterOutputTrigger,AutoReloadPreload,IC1Filter,Period,IC2Filter
TIM2.Period=ENCODER_MAX_COUNT
TIM2.TIM_MasterOutputTrigger=TIM_TRGO_RESET
TIM2.TIM_MasterSlaveMode=TIM_MASTERSLAVEMODE_DISABLE
TIM3.AutoReloadPreload=TIM_AUTORELOAD_PRELOAD_ENABLE
TIM3.IPParameters=Prescaler,Period,AutoReloadPreload
TIM3.Period=SAMPLING_TIM_PERIOD_COUNT
TIM3.Prescaler=SAMPLING_TIM_PRE
TIM4.AutoReloadPreload=TIM_AUTORELOAD_PRELOAD_ENABLE
TIM4.IPParameters=Prescaler,AutoReloadPreload,Period
TIM4.Period=US_TIM_PERIOD_COUNT
TIM4.Prescaler=US_TIM_PRE
UART5.BaudRate=9600
UART5.IPParameters=VirtualMode,BaudRate
UART5.VirtualMode=Asynchronous
USART1.IPParameters=VirtualMode
USART1.VirtualMode=VM_ASYNC
USART2.IPParameters=VirtualMode
USART2.VirtualMode=VM_ASYNC
USART3.BaudRate=57600
USART3.IPParameters=VirtualMode,BaudRate
USART3.VirtualMode=VM_ASYNC
VP_RealThread.X-CUBE-RT-Thread_Nano_VS_RTOSJjRTAaThread_4.1.1_4.1.1.Mode=RTOSJjRTAaThread
VP_RealThread.X-CUBE-RT-Thread_Nano_VS_RTOSJjRTAaThread_4.1.1_4.1.1.Signal=RealThread.X-CUBE-RT-Thread_Nano_VS_RTOSJjRTAaThread_4.1.1_4.1.1
VP_STMicroelectronics.X-CUBE-ALGOBUILD_VS_DSPOoLibraryJjLibrary_1.4.0_1.4.0.Mode=DSPOoLibraryJjLibrary
VP_STMicroelectronics.X-CUBE-ALGOBUILD_VS_DSPOoLibraryJjLibrary_1.4.0_1.4.0.Signal=STMicroelectronics.X-CUBE-ALGOBUILD_VS_DSPOoLibraryJjLibrary_1.4.0_1.4.0
VP_SYS_VS_tim8.Mode=TIM8
VP_SYS_VS_tim8.Signal=SYS_VS_tim8
VP_TIM3_VS_ClockSourceINT.Mode=Internal
VP_TIM3_VS_ClockSourceINT.Signal=TIM3_VS_ClockSourceINT
VP_TIM4_VS_ClockSourceINT.Mode=Internal
VP_TIM4_VS_ClockSourceINT.Signal=TIM4_VS_ClockSourceINT
board=custom
